INFAMOUS AERO CO. Graphical user interface, application

Description automatically generated

Ford Focus RS – V2 Front Splitter Chassis Mount Install

A picture containing car, transport, blue, curb

Description automatically generatedA picture containing grate

Description automatically generated

Kit Includes:

Infamous Aero V2 Splitter, Infamous Aero Chassis Mount Center Bracket, Infamous Aero Chassis Mount Side Bracket (x2), Infamous Aero Decals (x2), Infamous Aero Gel Badge, M8x30 Bolts (x8), M8 Fender Washers (x16), and M8 Locking Nuts (x8).

Necessary Tools:

Panel Clip Remover (Flat Head Screwdriver), 13mm Wrench, 10mm Wrench, ¼” Rachet, ½” Rachet, 13mm Socket, 10mm Socket, Torques bit, Drill, and Drill Bits.

A picture containing text, wall, indoor

Description automatically generated

Step 1: Remove Front Bumper & Headlights

A picture containing blue, plastic, engine

Description automatically generatedA close-up of a car engine

Description automatically generated with medium confidence

A picture containing blue

Description automatically generatedA close-up of a car

Description automatically generated with low confidence

Remove/disconnect all highlighted hardware, both sides.

Step 2: Remove Air Dams

The front of a car

Description automatically generated with low confidence

Step 3: Drill Factory Mounting Location

A picture containing blue

Description automatically generatedA close-up of a machine

Description automatically generated with medium confidence

Both sides with 11/32nd drill bit.

Step 4: Install Center Bracket – Check Clearance



May require remounting bumper to ensure splitter is set at correct height. Use height adjustment bolts on center bracket as necessary.

Step 5: Mark Two Front Hole Locations on Splitter

Once center bracket is mounted at correct height mark front two-hole locations on Infamous Aero Front Splitter.

Step 6: Remove Center Backet & Fully Mount Splitter to Center Bracket

A picture containing outdoor

Description automatically generated

Mark and drill remaining three holes on center bracket. \*Drill down if splitter includes carbon overlay option.

Step 7: Re-Install Center Bracket & Side Brackets

A picture containing transport, car

Description automatically generatedA picture containing engine

Description automatically generatedA close-up of a machine

Description automatically generated with low confidenceA close-up of a machine

Description automatically generated with low confidence

Side brackets can be installed once center bracket is fully mounted and in its final position using OEM bolt and bolt location. Ensure provided fender washers are used on front and back of center bracket mounting locations.

Step 8: Re-Install Air Dams

A close-up of a blue vehicle

Description automatically generated with low confidence

INFAMOUS AERO Bracket System does not require deleting any factory panels or air dams.

Step 9: Re-Install Front Bumper

A picture containing blue, transport, car

Description automatically generatedA picture containing car, ground, blue, parked

Description automatically generated

Thank-you for your support and Welcome to the INFAMOUS AERO TEAM.

If you have any further questions do not hesitate to contact [info@infamousaero.com](mailto:info@infamousaero.com).